Top Surface-Premium Worktops

Here are some of the things that you can take away with you from our shop!

### QUARTZ

###### Premium quartz

Tips:

1. Use trivets for hot pots - quartz is heat-resistant, but not heat-proof.
2. Clean with mild soap and water - avoid abrasive or bleach-based cleaners.
3. Don't cut directly on the surface - it can scratch with heavy use.
4. Avoid prolonged sunlight exposure - UV can discolor some quartz brands

Installation Advice:

- Ensure accurate measurements before ordering.
- Use adequate bracing to prevent bracing.
- Avoid On-Site Modifications.

### MARBLE

###### Premium marble

Tips:

1. Seal regularly (every 6-12 months) to reduce staining risk.
2. Avoid acidic substances (lemon, vinegar, wine) - they can etch the surface.
3. Clean with pH-neutral stone cleaner or warm water and mild soap.
4. Don't use abrasive pads - they'll dull the polish.

Installation Advice:

- Professional Installation Required
- Use a Stable, Level Base
- Seal Immediately After Fitting

### LAMINATE

###### Premium laminate

Tips:

1. Use non-abrasive cleaners - harsh chemicals can damage the finish.
2. Always use a cutting board - laminate scratches easily.
3. Wipe up water quickly - seams can swell or delaminate if moisture seeps in.
4. Never place hot pans directly on it - use heat pads or trivets.

Installation Advice:

- DIY-Friendly
- Seal Joints Properly
- Use Contact Adhesive

### SOLID SURFACE

###### Premium solid surface

Tips:

1. Minor scratches can be buffed or sanded out with a Scotch-Brite pad.
2. Keep it dry when not in use - although non-porous, it helps maintain sheen.
3. Avoid direct heat - like quartz, it can warp or discolor.
4. Regular cleaning with a damp cloth and mild soap keeps it looking new.

Installation Advice:

- Acclimatize Before Fitting
- Use Expansion Gaps
- Oil Immediately After Installation

### WOODEN

###### Premium wooden

Tips:

1. Oil regularly (monthly) with food-safe mineral oil to prevent drying/cracking.
2. Clean spills promptly - wood is porous and can stain or harbor bacteria.
3. Accepts cutting, but consider using a board to extend its life.
4. Sand and refinish if damaged - one of the most repairable surfaces

Installation Advice:

- Secure with Slotted Brackets
- Check Moisture Content
- Support Around Cut-Outs

#### Comparison table

Worktop Type | Durability | Maintenance | Price Range | Heat Resistant
--- | --- | --- | --- | ---
Wooden | Very High | Low | $135 | Medium
Marble | Very High | Low | $170 | High
Laminate | Medium | Low | $65 | Low
Quartz | High | Low | $150 | Medium
Solid Surface | Medium | Medium | $70 | Medium