# Symmetrical Drilling

Symmetric is a system comprised of an ingeniously simple concentric method of drilling through overburden with casing. Symmetric can drill straight holes at any angle (including horizontal) and to depths beyond 100 meters.It is a specialized techinique used for drilling larg diameter boreholes in challenging Geological conditions

###### Symmetrical One

###### Symmetrical two

###### Symmetrical three

###### Symmetrical Four

# Core Drilling

Core drilling is the process of using a hollow drill to drll holes through certain surfaces.It's a highly reccommended metod provided its faster work output compared to the rest.

###### Why core drilling:

- It is an important step for any project
- It gets more accurate samples that can get you in4 about your place of stay

###### Pavements core driller

###### Labaratory core driller Machine

###### Portable Core Drilling Machine

###### Universal Core Drilling Machine

# Geotechnical Drilling

Geotechnical drilling is a specialized and critical method to study and explore the materials beneath the ground. It involves drilling into the ground to obtain information about the soil and rock layers beneath the surface. This information is crucial for understanding the geological conditions of a job site, which is essential for safe and efficient construction, mining, and environmental projects. Geotechnical drilling plays a vital role in this understanding. It helps assess the ground’s stability, strength, and physical properties, ensuring drillers build structures on solid foundations. This process is essential in planning any construction project because it prevents unpredictable complications that could arise due to unknown subsurface conditions.

###### Rotary Drilling

This fast drilling technique uses a rotary motion to drill into the Earth. It's ideal for penetrating through hard rock layers, drilling large holes, obtaining rock samples for deep observation, and gathering information about coal deposits

###### Core Drilling

Core drilling extracts a cylindrical sample of the ground material, providing valuable information about the soil and rock layers. This information is crucial for building foundations, bridges, and tunnels

###### Mud Rotary Drilling

This technique, known for its speed and adaptability, circulates drilling mud fluid to remove drill cuttings from the hole. This method is effective for coring bedrock and keeping the borehole stable.

##### About Us

Kadendi Boreholes & Drilling Co. is a fully registered borehole drilling company in kenya registered under the Companies Act (Cap.486). with its headquarters in Nairobi, started in the year 2010 to provide reliable water services. Following the drastic climate change being experienced in the world, normal rainfall has become highly unrealiable and unpredictable thus the need for an alternative.

We have a team of both water and civil engineers with a wealth of experience in borehole drilling and other water services in kenya and abroad. We take time to listen to our client's water requirements then propose a solution which can either be a borehole, geo-Membrane ponds, shallow wells or elevated tanks depending on the budget.

##### Contact Us

##### Stay Connected

we can also be found on the above social media platforms.For more information please reach to us and enjoy our services.

#### Thank You for visiting the site